Transmit pattern:

 

 
transmit_pattern object
 
          stdValues: [1x1 struct]
           Voltages: []
           aprtArea: ' cm^2'
            aprtDim: '[, '
     activeElements: '1: [1, 1]'
       transmitFreq: '1.0 MHz'
              focus: '[, '
          numcycles: []
           polarity: []
    termPulseLength: []
               mode: []
      scanDirection: []
                PRF: 1000
            TXdelay: 0
                DOF: ' mm'
         breakPoint: '0.0 mm'
         coordTrafo: [4x4 double]
              scans: {1x3 cell}
            comment: {''}
           saveFile: []
              depth: []



Scans:

1 beamProfileScan   2010-05-06 14:33:13 15V
2 beamProfileScan   2010-05-06 14:33:58 15V
3 beamProfileScan   2010-05-06 15:01:25 16V
